Third, the Communication between controller and server is done through USB port and it is serial communication we need to adjust the Buad rate to 9600 bps and specify the correct port no to establish the connection with the controller . then the communication consists of serial messages between the Arduino controller and the server each party would decode the message and translate it to the corresponding action